**Micronics Technology H89 ESP32 Interface Status Update**

**Darrell Pelan**

**11 Apr 2022**

* Initial PCB design complete
* This card is installed inside the Heathkit H-89 in the rightmost bus slot (H17 floppy disk controller location)
* Current design uses ESP32 Dev kit and plug in Micro SD Card module. Future designs will use a surface mount ESP32, micro USB socket, and micro SD card socket that will allow better placement of the ESP32 antenna, USB and micro SD sockets.
* Board size
  + 116 mm x 124 mm

A picture containing text, electronics, screenshot

Description automatically generated

A screenshot of a computer

Description automatically generated with medium confidence